For 1990-2009 cars

#### Special Tools

KM-6351 Assembly Sleeves

1. Clean the sealing surfaces.
2. Slide the KM-6351 (2) protective sleeve onto the crankshaft journal.
3. Slide the crankshaft front oil seal over the protective sleeve on the crankshaft journal.
4. Remove the protective sleeve, and using the KM-6351 (3), press the seal ring into the pump housing.
5. Use the crankshaft drive gear bolt (1) and washer (2) to press in the crankshaft front oil seal.