For 1990-2009 cars

### Removal Procedure

1. Remove the heater/air conditioning control. Refer to Heater and Air Conditioning Control Replacement.
2. Remove the instrument panel (I/P) padding cover.

• | Remove the 2 bolts (1).

• | Remove the panel.

• | Disconnect the wiring harness plug (2).

• | Release the wiring harness plug and disconnect.

3. Remove the accessory switch.

Release the 2 locks (1).

### Installation Procedure

1. Install the accessory switch.

Release the 2 locks.

2. Install the I/P padding cover.

• | Connect the wiring harness plug.

• | Install the panel.

Tighten
Tighten the 2 screws.

3. Fit heater/air conditioning unit control. Refer to Heater and Air Conditioning Control Replacement.