For 1990-2009 cars

#### Special Tools

KM-845 Suction Device

### Removal Procedure

1. Remove the camshafts. Refer to Camshaft Replacement .

Important: Mark assignments.

2. Remove the 16 cup tappets with KM-845 (1).

### Installation Procedure

Important: Observe correct assignment.

1. Insert the 16 cup tappets with KM-845 (1).

Lightly coat sliding surfaces with engine oil.

2. Install the camshafts. Refer to Camshaft Replacement .