For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat head restraint.

• | Press in the retaining clamp.

• | Remove the head restraint upwards.

Important: Position I shows the lug to the right of the head restraint guide sleeve which must be pushed in for removal.

2. Remove the head restraint guide sleeve (1).

• | Push the guide sleeve (1) upwards with a suitable tool (e.g. pointed pliers) and compress both lugs (2) upwards with a screwdriver at the same time.

• | Pull the guide sleeves upwards off of the rear seat backrest.

### Installation Procedure

1. Push the guide sleeve into the rear seat backrest until it engages.
2. Install the headrest

Engage the head restraint (audible click).