For 1990-2009 cars

#### Special Tools

• | KM-422 Installer

• | KM-J-45000 Remover

### Removal Procedure

Important: Do not damage sealing surfaces.

1. Remove the intake camshaft adjuster or the exhaust camshaft adjuster. Refer to Camshaft Position Intake Actuator Replacement or Camshaft Position Exhaust Actuator Replacement .
2. Remove the camshaft seal ring (1) with KM-J-45000 (2).

### Installation Procedure

1. Insert the camshaft seal ring.

• | Install the seal ring with KM-422 (3).

• | To install, use the camshaft adjuster (1) in conjunction with shims (2) with a total thickness of approximately 10 mm (0.39 in).

• | Remove KM-422 .

• | Remove the bolt.

2. Install the intake camshaft adjuster or the exhaust camshaft adjuster. Refer to Camshaft Position Intake Actuator Replacement or Camshaft Position Exhaust Actuator Replacement .