For 1990-2009 cars

Table 1: | DIS Scan Tool Data Parameters
Table 2: | DIS Scan Tool Output Controls

#### DIS Scan Tool Data Parameters

Parameter | System State | Expected Value | Description
--- | --- | --- | ---
Operating Conditions: Ignition ON
Car Key In Recognition | -- | Active 12V | The scan tool displays Inactive or Active 12V. Active 12V is displayed when the appropriate key is in the ignition.
Engine Coolant Temperature | -- | Varies | This displays °F (°C). This is the current estimated engine coolant temperature.
Fuel Level | -- | Varies | This displays L (liters) or Gal (gallons). This is the current estimated fuel remaining in the fuel tank.
Ignition Status | -- | On | The scan tool displays On or Off. This is the current status of the ignition.
Left Steering Wheel Remote Control Status | -- | No Key Pressed | The scan tool displays No Key Pressed, Up-Key, Down-Key, Menu Down, Menu Up or Pushed.
Outside Temperature | -- | Varies | This displays °F (°C). This is the current estimated outside air temperature.
Right Steering Wheel Remote Control Status | -- | No Key Pressed | The scan tool displays No Key Pressed, Up-Key, Down-Key, Volume Down or Volume Up.
Rotary EHU Button Status | -- | No Key Pressed | The scan tool displays No Key Pressed, Left, Right or Pushed.
Theft Protection | -- | ID O.K. | The scan tool displays Unit disabled, Delivery State, ID N.O.K. yet, ID-Comp running or ID O.K. This is the current state of the theft protection.
Vehicle Speed | -- | 0 km/h (0 mph) | This displays km/h (mph). This is the current speed of the vehicle.

#### DIS Scan Tool Output Controls

Output Control | Description
--- | ---
Display Test | This output control is used command the instrument panel gages or indicators.
Program Code Index | This output control is used to program the code index.
Program ECU | This output control is used to program the electronic control unit (ECU) or control module.
Program High Speed CAN-Bus Config. | This output control is used to program the high speed control area network (CAN) serial data bus configuration.
Program Low Speed CAN-Bus Config. | This output control is used to program the low speed control area network (CAN) serial data bus configuration.
Program Mid Speed CAN-Bus Config. | This output control is used to program the mid speed control area network (CAN) serial data bus configuration.
Program Variant Configuration | This output control is used to program the variant configuration.
Read Check Control Status | This output control is used to read the check control status.
Read ECU Identification | This output control is used to read the electronic control unit (ECU) or control module identification.
Reset ECU | This output control is used to reset the electronic control unit (ECU) or control module.
Set Time and Date | This output control is used to set the time and date.
Theft Protection without Radio | This output control is used to program the theft protection without the radio.