For 1990-2009 cars

### Removal Procedure

1. Fold down the center rear seat back cushion.
2. Remove the center rear seat back cushion latch striker.

Remove the latch striker.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the center rear seat back cushion latch striker.

Tighten
Tighten the latch striker to 60 N·m (44 lb ft).

2. Return the rear center seat back to original position.