For 1990-2009 cars

#### Special Tools

KM-652 Flywheel Holder

For equivalent regional tools, refer to Special Tools.

1. Install the flywheel.

Clean the thread in the crankshaft.

2. Using the KM-652 holder , hold the flywheel.

Caution: Refer to Fastener Caution in the Preface section.

3. Install NEW bolts. Tighten the 6 bolts to 35 N·m (26 lb ft) + 30 degrees+ 15 degrees.
4. Remove the KM-652 holder .