For 1990-2009 cars

### Removal Procedure

1. Remove the starter. Refer to Starter Motor Replacement.
2. Remove the crankshaft position sensor.

• | Disconnect the wiring harness plug (1).

• | Disconnect the crankshaft position sensor (2) from the bracket.

• | Remove the bolt (3).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the crankshaft position sensor.

Tighten
Tighten the bolt to 4.5 N·m (40 lb in).

• | Install the wiring harness plug into the bracket.

• | Install the wiring harness plug.

2. Install the starter. Refer to Starter Motor Replacement.