For 1990-2009 cars

### Removal Procedure

Important: To release the headlamp switch center, push in rotary switch (1) while the switch is in position "0", move the rotary switch to the center position (3) while it is pushed down, headlamp switch center (2) is now released.

1. Release the headlamp switch center.
2. Pull out the headlamp switch center.
3. Disconnect the wiring harness plug for the headlamp switch center.

• | Disconnect the wiring harness plug.

• | Push down the secondary retainer (2).

• | Release the retainer (1).

4. Remove the panel for the headlamp switch center.

Release 8 clips (arrows).

### Installation Procedure

1. Install the panel for the headlamp switch center.

Install 8 clips.

2. Connect the wiring harness plug for the headlamp switch center.
3. Insert the headlamp switch center.

Important: Turn the rotary switch (1) to position "0", the headlamp switch lock (2) comes out.

4. Lock the headlamp switch center.