For 1990-2009 cars

### Removal Procedure

1. Remove the protective cover from the inside remote control knob.
2. Remove the cover (1) from the upper extension trim panel.
3. Remove the upper extension trim panel (2).

Release the 3 clips.

4. Remove the remote control knob (1) from the manual mirror.

• | Remove the 2 bolts, (arrows).

• | Remove the mirror remote control knob.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the remote control knob to the manual mirror.

Insert the knob.

Tighten
Tighten the 2 bolts to 5 N·m (44 lb in).

2. Install the upper extension panel.

Install the 3 clips.

3. Install the protective cover to the upper extension panel.
4. Install the cover.