For 1990-2009 cars

# Infotainment System (Radio) Inoperative At PDI - keywords accessories amp audio body cd cd30 cd40 entertainment fuse infotainment inoperative MP3 PDI performance radio system

Subject: | Infotainment System (radio) Inoperative at PDI

Models: | 2008 Saturn Astra

The following diagnosis might be helpful if the vehicle exhibits the symptom(s) described in this PI.

### Condition/Concern:

A technician may find the Infotainment/radio system is inoperative when performing the PreDelivery Inspection (PDI).

### Recommendation/Instructions:

Due to the extended shipping time of the Astra the fuse for the Infotainment/radio system is moved to an empty cavity in the UHJB to lower power consumption during transit. Use a fuse puller to move the 20 amp Infotainment (radio) fuse from cavity F11 (See Illustration A Below) to cavity F35 in the under hood junction block (UHJB). The fuse puller is located in the rear zone module located on the left side of the cargo area behind a cover between the two large connectors in the middle (See Illustration B Below). This information is available in the 2008 Astra PDI form "Special Instruction Items" in DealerWorld and the new model features bulletin 07-00-89-058a in Service Information.

#### Illustration A

Green arrow (upper) is before shipment

Red arrow (lower) is after shipment

(1) Is location F11

(2) Is location F35

Note: To move the fuse a fuse puller is needed. The tool is located in the rear zone module.

#### Illustration B

(1) Is Fuse Puller Location

Please follow this diagnostic or repair process thoroughly and complete each step. If the condition exhibited is resolved without completing every step, the remaining steps do not need to be performed.