For 1990-2009 cars

Important:

• | Repair kit is suitable for repairs to pumps, spray nozzle or any part of the washer/wiper hose.

• | Remove the relevant panelling, if necessary.

1. Remove the air inlet screen. Refer to Air Inlet Screen Replacement .
2. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement .

Important: Cut through the hose in the valley (1).

3. Cut the washer/wiper system hose at the point of fracture.
4. Install the new rubber rings.

Attach the 2 rubber rings (arrow).

5. Prepare both ends of the hose.

Grease both rubber rings with silicone grease.

6. Insert the connector (1) and secure.

Attach the 2 securing elements (2).

7. Install the front bumper fascia. Refer to Front Bumper Fascia Replacement .
8. Install the air inlet screen. Refer to Air Inlet Screen Replacement .