For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Front Brakes

- Brake Pad Lining Minimum Thickness

2.0 mm

0.079 in

- Brake Pad Lining Thickness - New

12.0 mm

0.472 in

- Rotor Discard Thickness *

22.0 mm

0.867 in

- Rotor Thickness (new)

25.0 mm

0.984 in

- Rotor Maximum Allowable Lateral Runout

0.11 mm

0.005 in

- Rotor Maximum Allowable Scoring

0.04 mm

0.158 in

- Rotor Maximum Allowable Thickness Variation

0.025 mm

0.001 in

* All brake rotors have a discard dimension cast into them. Replace any rotor that does not meet this specification. After refinishing the rotor, replace any rotor that does not meet the minimum thickness specifications.