For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the battery.
2. Remove the fuel tank. Refer to Fuel Tank Replacement .

Important: The illustration shows the vehicle without attaching parts for a clearer representation.

3. Remove the wiring harness, fuel tank.

• | Disconnect the 4 wiring harness plugs.

• | Remove the wiring harness.

### Installation Procedure

1. Install the wiring harness, fuel tank.

• | Position the wiring harness.

• | Connect the 4 wiring harness plugs.

2. Install the fuel tank. Refer to Fuel Tank Replacement .
3. Connect the battery.
4. For programming procedures, refer to Control Module References .