For 1990-2009 cars

#### Special Tools

KM-6349 Fixing Rod

### Removal Procedure

1. Raise the vehicle by its full height.
2. Remove the lower engine cover and the right engine splash shield.
3. Remove the drive belt.

• | Apply tension to the drive belt tensioner in the direction of the arrow at the projection (1) and lock with KM-6349 (2).

• | Remove the drive belt.

### Installation Procedure

1. Install the drive belt.

• | Apply tension to the tensioner at the projection counterclockwise in the direction of the arrow.

• | Remove the KM-6349 .

• | Allow the tensioner to slide back slowly.

2. Install the lower engine cover and the right engine splash shield.
3. Lower the vehicle by its full height.