For 1990-2009 cars

### Removal Procedure

1. Release the panel for the microphone (2) and the panel for the sliding sunroof control unit (3).

Release using a suitable tool (screwdriver).

2. Remove the lens from the interior lamp (1).
3. Remove the front interior lamp holder.

• | Remove the 2 bolts (1).

• | Release the holder (4) all around.

• | Disconnect the wiring harness holder (2).

• | Disconnect the wiring harness plug (3).

4. Remove the switch with the theft deterrent sensors.

• | Disconnect the compact plug (1).

• | Release and disconnect the wiring harness at the compact plug (arrow).

• | Disconnect and remove the panel with the theft deterrent sensors (2).

### Installation Procedure

1. Install the switch with the theft deterrent sensors.

• | Install the panel with the theft deterrent sensors.

• | Insert the wiring harness in the compact plug and lock.

• | Connect the compact plug.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the front interior lamp holder.

• | Connect the wiring harness plug.

• | Connect the wiring harness holder.

• | Connect the holder all around.

Tighten
Tighten the 2 screws to 2.5 N·m (22 lb in).

3. Install the lens for the interior lamp.

Install the 4 clips.

4. Install the microphone panel and the panel for the sliding sunroof control unit.

Install the 2 panels.