For 1990-2009 cars

## Front Side Door Molding Replacement Sedan

### Removal Procedure

1. Remove the front door molding.

Carefully pry off the molding with a plastic wedge (1).

Important: Ensure that the paint is not damaged.

2. Remove the remaining adhesive.

Remove the remaining adhesive from the molding and door with a molding adhesive remover disk (2).

### Installation Procedure

1. Dimensions 5 door.

• | Front Clearance - Horizontal (I) 169 mm (6.65 in).

• | Rear Clearance - Vertical (II) 155 mm (6.10 in).

• | Front Clearance - Vertical (III) 143 mm (5.63 in).

Important: The adhesive surface must be grease and dust free.

2. Apply adhesive strips on the molding.
3. Install the front side door molding.

## Front Side Door Molding Replacement Coupe

### Removal Procedure

1. Remove the front side door molding.

Carefully pry off the molding with a plastic wedge (1).

Important: Ensure that the paint is not damaged.

2. Remove the remaining adhesive.

Remove the remaining adhesive from the molding and door with a molding adhesive remover disk (2).

### Installation Procedure

1. Dimensions 3 door.

• | Front Clearance--Horizontal (I) 233 mm (9.17 in).

• | Rear Clearance--Vertical (II) 187 mm (7.36 in).

• | Front Clearance--Vertical (III) 155 mm (6.10 in).

Important: The adhesive surface must be grease and dust free.

2. Apply adhesive strips on the molding.
3. Install the front side door molding.