For 1990-2009 cars

Each of the outside rearview mirrors contains two motors. The vertical motor operates the mirror in the up and down directions, and the horizontal motor operates the mirror in the left and right directions. Each of the outside rearview mirror motors are circuit breaker protected.

### Power Mirror System Controls

The outside rearview mirror switch is a four position directional switch: Up, Down, Left and Right.

The mirror select switch is a three position switch: Left, Neutral, and Right.

### Power Mirror System Operation

The outside rearview mirror switch receives power through the battery positive voltage circuit from the power mirror fuse. The power mirror switch also receives a constant ground.

The four positions of the direction switch have dual switch contacts. Each of the contacts are connected to opposing sides of the appropriate power mirror motors through the selector switch. The selector switch completes these circuits depending on the position of the selector switch, left or right.

If the selector switch is placed in the left position and the up switch is depressed, battery positive voltage will be supplied to the left outside rearview mirror vertical motor through the left mirror motor down control circuit and ground through the left mirror motor left control circuit. If the down switch is depressed, battery positive voltage will be supplied to the left outside rearview mirror vertical motor through the left mirror motor left control circuit and ground through the left mirror motor down control circuit.

The remainder of the mirror functions operate in the same manner as described above. Placing the power mirror switch in opposing positions, left/right or up/down, will reverse the polarity to the mirror motor, reversing the direction of movement.