For 1990-2009 cars

### Removal Procedure

Note: When replacing the control unit, before removing the control unit, carry out a Reset using the Tech 2. For reprogramming procedures, refer to Control Module References.

1. Remove the instrument panel (I/P) compartment.

1.1. | Remove the 4 bolts (1).

1.2. | Disconnect the wiring harness plug.

2. Remove the tire pressure indicator (1) receiver.

2.1. | Disconnect the pressure indicator receiver bracket (2) from the crossmember.

2.2. | Disconnect the wiring harness plug.

2.3. | Disconnect the indicator receiver from bracket.

### Installation Procedure

1. Install the tire pressure indicator receiver.

1.1. | Install the indicator receiver into the bracket.

1.2. | Connect the wiring harness plugs.

1.3. | Install the indicator receiver bracket to the crossmember.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the I/P compartment.

Connect the wiring harness plugs.

Tighten
Tighten the 4 bolts to 4 N·m (35 lb in).

3. For programming procedures, refer to Control Module References.