For 1990-2009 cars

### Removal Procedure

1. Open the hood.
2. Place a drain pan underneath.
3. Disconnect the wiring harness from the cylinder head.
4. Remove the 2 valves, camshaft position actuator solenoid (3).

• | Disconnect the 2 wiring harness plugs (1).

• | Remove the 2 bolts (2).

• | Remove the 2 camshaft position actuator solenoid valves from the bearing support.

### Installation Procedure

1. Install the 2 valves, camshaft position actuator solenoid.

• | Insert the 2 camshaft position actuator solenoid valves all the way.

• | Coat the seal rings with clean engine oil.

Notice: Refer to Fastener Notice in the Preface section.

• | Tighten the 2 bolts.

Tighten
Tighten the 2 bolts to 6 N·m (53 lb in).

• | Connect the 2 wiring harness plugs.

2. Connect the wiring harness to the cylinder head.
3. Inspect the engine oil level and correct if necessary.
4. Close the hood.