For 1990-2009 cars

### Removal Procedure

Remove the front grille speaker.

• | Remove the grille for the speaker (1).

• | Remove the ambient light sensor.

• | Remove the defroster panel (5) and unscrew the underlying bolt.

• | Remove the bolt (4).

• | Remove the front speaker.

• | Disconnect the wiring harness plug.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

Install the front speaker.

• | Insert the front speaker.

• | Connect the wiring harness plug.

Tighten
Tighten the 2 screws to 4 N·m (35 lb in).

• | Install the defroster panel.

• | Install the ambient light sensor.

• | Install the front speaker grille.