For 1990-2009 cars

### Removal Procedure

1. Remove the front-side door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the front door speaker.

Remove the 3 bolts (arrows).

3. Disconnect the wiring harness plug for the front door speaker.

### Installation Procedure

1. Connect the wiring harness plug for the front door speaker.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the front door speaker.

Tighten
Tighten the 3 bolts to 2.5 N·m (22 lb in).

3. Install the front door inner panel. Refer to Front Side Door Trim Panel Replacement .