For 1990-2009 cars

### Removal Procedure

1. Remove the rear side door molding.

Carefully remove the molding with a plastic wedge (1).

Important: Ensure that the paint is not damaged.

2. Remove the remaining adhesive from the molding and door with a molding adhesive remover disk (2).

### Installation Procedure

1. Dimensions 5 door.

• | Front Clearance--Horizontal (I) 3 mm (0.12 in).

• | Rear Clearance--Vertical (II) 160 mm (6.30 in).

• | Front Clearance--Vertical (III) 155 mm (6.10 in).

Important: The adhesive surface must be grease and dust free.

2. Apply adhesive strips on the molding.
3. Install the rear side door molding.