For 1990-2009 cars

### Removal Procedure

1. Remove the front fender liner.

Remove the 2 bolts (1).

2. Remove the front fender liner.

Remove the 8 body-bound rivets (arrows).

### Installation Procedure

1. Install the front fender liner.

Install the 8 body-bound rivets.

Notice: Refer to Fastener Notice in the Preface section.

2. Fasten the front fender liner.

Tighten
Tighten the 2 bolts to 2.5 N·m (22 lb in).