For 1990-2009 cars

### Removal Procedure

1. Remove the upper fascia grille.

• | Remove the 4 bolts (1).

• | Remove the 7 retainers (2).

2. When replacing the upper fascia grille, transfer the attaching parts.

### Installation Procedure

1. Install the upper fascia grille.

Install the 7 retainers.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the upper fascia grille bolts.

Tighten
Tighten the 4 bolts to 2.5 N·m (22 lb in).