For 1990-2009 cars

To open the liftgate, See Liftgate .

The rear compartment fuse block is located on the left side of the cargo area behind a cover.

Use the fuse puller, to remove and replace fuses.

Fuses | Usage
--- | ---
1 | Front Power Window
3 | Cluster
4 | Climate Control System (Battery)
11 | Rear Defogger
12 | Rear Windshield Wiper
14 | Climate Control System (Ignition)
16 | Front Passenger Seat Detection Sensor
17 | Tire Pressure Monitoring System (TPMS)/Rain Sensor/Inside Rearview Mirror
18 | Interior Lights
21 | Outside Mirror Heating
22 | Sunroof
23 | Rear Power Window
24 | Diagnostic Link Connector
29 | Accessory Power Outlet (APO)
34 | Sunroof
38 | Door Locks
39 | Seat Heating Driver
40 | Seat Heating Front Passenger