For 1990-2009 cars

## Rear Bumper Fascia Center Support Replacement Coupe

### Removal Procedure

1. Remove the rear bumper fascia. Refer to Rear Bumper Fascia Replacement .
2. Remove the center support.

Drill out the 3 blind rivets (arrows).

3. Remove the wiring harness.

Release the 2 cable ties (1).

4. On vehicles with park pilot, release the wiring harness plug (2) from the bracket.

### Installation Procedure

1. Install the center support.

Rivet on the 3 blind rivets.

2. On vehicles with park pilot, fasten the wiring harness plug to the bracket.
3. Install the wiring harness.

Connect the 2 cable ties.

4. Install the rear bumper fascia. Refer to Rear Bumper Fascia Replacement .

## Rear Bumper Fascia Center Support Replacement Sedan

### Removal Procedure

1. Remove the rear bumper fascia. Refer to Rear Bumper Fascia Replacement .
2. Remove the center support.

Drill out the 5 blind rivets (arrows).

3. Remove the wiring harness.

Release the 2 cable ties.

4. Remove the bracket from wiring harness plug (1).
5. On vehicles with park pilot, release the wiring harness plug from the bracket.

### Installation Procedure

1. Install the center support.

Rivet on the 5 blind rivets.

2. Install the bracket for the wiring harness plug.
3. Install the wiring harness.

Install the 2 cable ties.

4. On vehicles with park pilot, fasten the wiring harness plug to the bracket.
5. Install the rear bumper fascia. Refer to Rear Bumper Fascia Replacement .