For 1990-2009 cars

### Removal Procedure

1. Remove the seat back cushion adjustment handle.

Release the handle (1) upwards.

2. Remove the seat back cushion release panel.

• | Release the 4 lugs with a suitable tool.

• | Remove upwards.

### Installation Procedure

1. Install the seat back cushion release panel.

• | Install the 4 lugs with a suitable tool.

• | Install upwards.

2. Install the seat back cushion adjustment handle.

Install the handle.