For 1990-2009 cars

#### Special Tools

KM-6625 Flywheel Locking Device

### Removal Procedure

1. Open the hood.
2. Disconnect the battery.

• | Disconnect the negative connection from the ground terminal.

• | Loosen the nut.

3. Raise the vehicle by its full height.
4. Remove the drive belt tensioner. Refer to Drive Belt Tensioner Replacement.
5. Block the crankshaft.

Attach KM-6625 .

• | Detach the screwed connection (1).

• | Insert KM-6625 (2).

• | Tighten the screwed connection (3).

6. Remove the torsional vibration damper (1).

Remove the bolt (2).

7. Remove the front toothed belt cover (bottom) (3).

Remove the 4 bolts (4).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the front toothed belt cover (lower).

Tighten
Tighten the 4 bolts to 6 N·m (53 lb in).

Note: The new bolt must be coated with screw locking compound (red).

2. Install the torsional vibration balancer.

Use a new bolt.

Tighten
Tighten the bolt to 95 N·m (70 lb ft) plus 30 degrees plus 15 degrees.

3. Remove KM-6625 .

• | Detach the screwed connection.

• | Tighten the bolted connection.

• | Use new nuts.

4. Lower the vehicle by its full height.
5. Install the drive belt tensioner. Refer to Drive Belt Tensioner Replacement.
6. Lower the vehicle by its full height.
7. Connect the battery.

Connect the negative connection to ground terminal.

Tighten
Tighten the nut to 5 N·m (44 lb in).

8. For programming procedures, refer to Control Module References.
9. Close the hood.