For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Catalytic Converter Monitoring Devise Oxygen Sensor | 40 N·m | 30 lb ft
Catalytic Converter to Bracket Bolts | 20 N·m | 15 lb ft
Compressor Bolts | 22 N·m | 16 lb ft
Engine Transport Shackle Bolts | 25 N·m | 18 lb in
Exhaust Heat Shield Nut - Front | 6 N·m | 53 lb ft
Exhaust Heat Shield Nut - Rear | 6 N·m | 53 lb ft
Exhaust Manifold Nuts | 20 N·m | 15 lb ft
Front Exhaust Pipe/Auxiliary Catalytic Converter Nut | 20 N·m | 15 lb ft
Front Exhaust Pipe/Auxiliary Catalytic Converter to Center Muffler Clamp | 50 N·m | 37 lb ft
Front Exhaust Pipe to Catalytic Converter Nuts | 20 N·m | 15 lb ft
Ground Terminal to Negative Connection Nut | 4 N·m | 44 lb in
Heat Shield to Catalytic Converter Bolts | 8 N·m | 70 lb in
Muffler Fastening Clamp Nut | 50 N·m | 37 lb ft
Oxygen Sensor | 30 N·m | 22 lb ft
Rear Muffler Fastening Clamp Nut | 50 N·m | 37 lb ft
Wiring Harness Bracket Bolt | 15 N·m | 11 lb ft
Wiring Harness to Mixture Regulator Oxygen Sensor Bracket Bolt | 25 N·m | 18 lb ft