For 1990-2009 cars

## Rear Window Washer Nozzle Replacement Sedan

### Removal Procedure

1. Remove the liftgate upper trim panel.
2. Remove the high mounted stop lamp.

Release the 6 clips (1).

3. Remove the high mounted stop lamp.

• | Disconnect the wiring harness plug (2) and remove.

• | Remove the hose (3) from the washer/wiper system.

4. Remove the washer nozzle (1).

### Installation Procedure

1. Install the washer nozzle.
2. Install the high mounted stop lamp.

• | Connect the hose for the washer/wiper system.

• | Connect the wiring harness plug.

• | Install the 6 clips.

3. Install the liftgate upper trim panel.

## Rear Window Washer Nozzle Replacement Coupe

### Removal Procedure

1. Remove the liftgate garnish molding. Refer to Liftgate Garnish Molding Replacement .
2. Release the high mounted stop lamp.

Release 3 guides (1).

3. Close the liftgate.
4. Remove the high mounted stop lamp.

• | Remove the hose from the washer/wiper system (4).

• | Disconnect the wiring harness (3).

• | Release the wiring harness plug (1, 2) and disconnect.

5. Remove the nozzle.

• | Disconnect the 2 retaining lugs (1).

• | Remove the spray nozzle.

### Installation Procedure

Important: Ensure correct installation position. Right-Left.

1. Install the nozzle.
2. Insert the high mounted stop lamp.

• | Connect and lock the wiring harness plug.

• | Connect the wiring harness.

• | Connect the hose for the washer/wiper system.

Notice: Refer to Fastener Notice in the Preface section.

Important: Be careful of the wiring harness plug when installing the brake light. Start from the right hand side.

Important: The high mounted stop lamp must engage audibly

3. Tighten the high mounted stop lamp.
4. Install the liftgate garnish molding, left and right. Refer to Liftgate Garnish Molding Replacement .