For 1990-2009 cars

### Removal Procedure

1. Remove the pad, front seat backrest. Refer to Front Seat Back Cushion Pad Replacement.
2. Remove the cushion pad support.

• | Remove the bolt.

• | Release the panel (1).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the cushion pad support.

Install the panel.

Tighten
Tighten the bolt to 3 N·m (26 lb in).

2. Install the pad, front seat backrest. Refer to Front Seat Back Cushion Pad Replacement.