For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (I/P) compartment.

1.1. | Remove the 4 bolts (1).

1.2. | Disconnect the wiring harness plug.

2. Remove the passenger side lower footwell trim.

Remove the bolt (3).

3. Remove the air duct.

Remove the body-bound rivet (2).

4. Remove the blower motor (2).

4.1. | Disconnect the 2 wiring harness plugs (1) from series resistor.

4.2. | Remove the 5 bolts.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the blower motor.

1.1. | Connect the clip.

Tighten
Tighten the 5 bolts to 6 N·m (63 lb in).

1.2. | Connect the 2 wiring harness plugs.

2. Install the air duct.

Install the body-bound rivet.

3. Install the lower right footwell trim.

Tighten
Tighten the bolt - pivot and lock.

4. Install the I/P compartment.

Connect the wiring harness plug.

Tighten
Tighten the 4 bolts to 4 N·m (35 lb in).