For 1990-2009 cars

### Removal Procedure

Important: In the presence of fuel vapors or escaping fuel, observe safety regulations and national legislation. Store drained fuel in a suitable, sealable container.

1. Open the fuel tank filler door.
2. Disconnect the release pull on the servo motor (1).

• | Open the fuel filler door.

• | Disconnect the bracket with the release pull in the direction of the arrow.

3. Open the fuel filler door.
4. Remove the stop with the release pull.

Remove the 2 bolts (1)

5. Remove the release pull from the fuel filler door stop.

### Installation Procedure

1. Install the release pull to the fuel filler door stop.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the stop with release pull.

Tighten
Tighten the 2 bolts to 1 N·m (9 lb in).

3. Close the fuel filler door.
4. Install the release pull on the servo motor.

• | Install the bracket with release pull.

• | Close the assembly flap.

5. Close the fuel filler door.