For 1990-2009 cars

#### Special Tools

• | KM-446 Installer Drift

• | KM-557-A /KM-557-2 Remover

### Removal Procedure

1. Remove the axle shaft. Refer to Wheel Drive Shaft Replacement .

Important: Do not damage the sealing surfaces.

2. Remove the axle shaft seal ring.

Remove the axle shaft seal ring with KM-557-A (2) and KM-557-2 (1).

### Installation Procedure

1. Install the axle shaft seal ring.

• | Coat the axle shaft seal ring with transmission fluid.

• | Install the axle shaft seal ring flush with KM-446 (1).

2. Install the axle shaft. Refer to Wheel Drive Shaft Replacement .
3. Inspect the transmission fluid level. Refer to Transmission Fluid Check .