For 1990-2009 cars

## Radio Antenna Replacement L08

### Removal Procedure

1. Lower the headlining trim panel. Refer to Headlining Trim Panel Replacement.
2. Remove the rear roof antenna.

• | Disconnect the wiring harness plug (1).

• | Remove the nut (2).

• | Remove the roof antenna.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the roof antenna.

Guide the wiring harness through fastening nut.

Tighten
Tighten the nut to 5 N·m (44 lb in).

2. Connect the roof antenna wiring harness.
3. Install the headlining. Refer to Headlining Trim Panel Replacement.

## Radio Antenna Replacement L48

### Removal Procedure

1. Remove the headlining trim panel. Refer to Headlining Trim Panel Replacement.
2. Remove the roof antenna.

• | Remove the roof antenna wiring harness plug (1).

• | Remove the nut.

• | Disconnect the wiring harness.

• | Remove the roof antenna.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the roof antenna.

Guide the wiring harness through fastening nut.

Tighten
Tighten the nut to 5 N·m (44 lb in).

2. Connect the roof antenna wiring harness.
3. Install the headlining trim panel. Refer to Headlining Trim Panel Replacement.
4. For reprogramming procedures, refer to Control Module References.