For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the battery.
2. Remove the battery shield.

• | Remove the bolt (3).

• | Remove the 2 shields (1) from the battery carrier.

3. Remove the battery holder (1).

Remove the bolt.

4. Remove the battery.
5. Remove battery carrier.

• | Disconnect the 2 cable ties (1).

• | Remove the 3 bolts (2).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the battery carrier.

Tighten
Tighten the 3 bolts to 15 N·m (11 lb ft).

2. Install the 2 cable ties.
3. Insert the battery.
4. Install the battery shield.

Install the 2 shield, battery carrier.

Tighten
Tighten the bolt to 10 N·m (89 lb in).

5. Install the battery holder.

Tighten
Tighten the bolt to 7 N·m (62 lb in).

6. Connect the battery.

• | Connect the positive cable.

• | Connect the ground cable.

7. For programming procedures, refer to Control Module References .