For 1990-2009 cars

### Removal Procedure

Warning: When working with any type of glass or sheet metal with exposed or rough edges, wear approved safety glasses and gloves in order to reduce the chance of personal injury.

Note: Only for power mirrors.

1. Remove the mirror glass.
2. Position the mirror face forward.
3. Position the mirror glass into the top right, left door, or the top left , right door.
4. Carefully pry out the mirror glass with a plastic wedge.
5. Remove the wiring harness plug for the mirror heating (1).

### Installation Procedure

1. Install the mirror glass.
2. Install the wiring harness plug.
3. Position and install the mirror glass in the mirror.
4. Position the mirror back to the original position.