For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the battery.
2. Wait 1 minute for the airbag to deactivate.
3. Remove the upper radiator grille. Refer to Front Bumper Upper Fascia Grille Replacement .
4. Remove the airbag sensor.

• | Loosen the 2 bolts (1).

• | Remove the airbag sensor from the guide.

• | Disconnect the wiring harness plug (2).

### Installation Procedure

1. Install the airbag sensor.

• | Connect the wiring harness plug.

Notice: Refer to Fastener Notice in the Preface section.

• | Insert the airbag sensor in the guide.

Tighten
Tighten the 2 bolts to 6 N·m (53 lb in).

2. Install the upper radiator grille. Refer to Front Bumper Upper Fascia Grille Replacement .
3. Connect the battery.
4. For programming procedures, refer to Control Module References .