For 1990-2009 cars
(Lock): Press to lock the doors, liftgate and fuel tank door. If the driver door is open, the doors will not lock.
(Unlock): Press to unlock the doors, liftgate and fuel tank door.

Press and hold to lower all the windows.

### Programming Transmitters to the Vehicle

Only RKE transmitters programmed to this vehicle will work. If a transmitter is lost or stolen, a replacement can be purchased and programmed through your dealer/retailer. When the replacement transmitter is programmed to this vehicle, all remaining transmitters must also be reprogrammed. Any lost or stolen transmitters will no longer work once the new transmitter is programmed. Each vehicle can have up to five transmitters programmed to it.

### Battery Replacement

Replace the battery if the Remote Control Battery check message appears in the DIC. See "Remote Control Battery Check" under DIC Warnings and Messages .

Notice: When replacing the battery, do not touch any of the circuitry on the transmitter. Static from your body could damage the transmitter.

To replace the battery:

1. Extend the key. See Keys for additional information.
2. Open the RKE transmitter.
3. Remove the old battery. Do not use a metal object.
4. Insert the new battery, positive side facing up. Replace with a CR2032 or equivalent battery.
5. Close the RKE transmitter.

### Synchronization

After changing the battery, turn the ignition to ON/RUN. This synchronizes the key.