For 1990-2009 cars

#### Special Tools

KM-652 Flywheel Holding Tool

### Removal Procedure

1. Remove the automatic transmission.
2. Detach the drive disc.

• | Lock the drive disc via starter ring gear with KM-652 (1).

• | Remove the 6 bolts.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Attach the drive disc.

• | Clean thread in crankshaft.

• | Use new bolts.

Tighten
Tighten the 6 bolts to 60 N·m (44 lb ft).

• | Remove KM-652 .

2. Install the automatic transmission.