For 1990-2009 cars

## Shoulder Belt Guide Bracket Replacement Coupe

### Removal Procedure

1. Remove the rear quarter lower trim. Refer to Quarter Lower Rear Trim Panel Replacement.
2. Remove the seat belt guide bracket.

Remove the 2 bolts, arrows.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the seat belt guide bracket.

Tighten
Tighten the 2 bolts to 1.5 N·m (13 lb in).

2. Install the rear quarter lower trim. Refer to Quarter Lower Rear Trim Panel Replacement.

## Shoulder Belt Guide Bracket Replacement Sedan

### Removal Procedure

1. Remove the upper center pillar garnish molding. Refer to Center Pillar Upper Garnish Molding Replacement.
2. Remove the seat belt guide bracket (2).

Remove the bolt (1).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the seat belt guide bracket.

Tighten
Tighten the bolt to 1.5 N·m (13 lb in).

2. Install the upper center pillar garnish molding. Refer to Center Pillar Upper Garnish Molding Replacement.