For 1990-2009 cars

## Rear Washer Hose Replacement Coupe

### Removal Procedure

1. Remove the luggage shade from the liftgate.

Disconnect the 2 retaining cords.

2. Remove the liftgate garnish moldings (1) on the upper left and right.

• | Remove the 2 luggage shade brackets (2).

• | Release the 6 clips.

3. Remove the rear quarter lower trim panel. Refer to Quarter Lower Rear Trim Panel Replacement .
4. Lower the headlining. Refer to Headlining Trim Panel Replacement .
5. Release the high mounted stop lamp.

Release the 3 retainers (1).

6. Remove the high mounted stop lamp.

• | Remove the hose from the stop lamp (4).

• | Disconnect the wiring harness (3).

• | Release the wiring harness plug (1, 2) and disconnect.

7. Disconnect and remove the hose.

• | Disconnect the hose at the center pillar (1).

• | Remove the hose.

• | Release the 5 clips (2, 3).

8. Remove the boot at the liftgate.

Disconnect the 2 retaining lugs (1).

9. Remove the hose.

• | Secure the new hose to the old hose with adhesive tape.

• | Remove the old hose.

• | Pull the new hose.

### Installation Procedure

1. Install the hose.

• | Route the hose.

• | Install the 5 clips.

• | Connect the hose at the center pillar.

• | Insert the boot.

• | Lock in the 2 retaining lugs.

2. Insert the high mounted stop lamp.

• | Connect and lock the wiring harness plug.

• | Connect the wiring harness.

• | Connect the hose for the washer/wiper system.

3. Fasten the third brake light.

Important:

• | Be careful of the wiring harness plug when installing the brake light. Install the high mounted stop lamp. Start from the right hand side.

• | The brake light must audibly engage.

4. Install the high mounted stop lamp.
5. Install the headlining. Refer to Headlining Trim Panel Replacement .
6. Install the rear quarter lower trim panel. Refer to Quarter Lower Rear Trim Panel Replacement .
7. Insert the garnish moldings, left and right.

• | Install the 6 clips.

• | Install the 2 luggage shade brackets.

8. Install the luggage shade to the liftgate.

Connect the 2 retaining cords.

## Rear Washer Hose Replacement Sedan

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the battery.
2. Remove the liftgate garnish molding - left side.

• | Remove the luggage shade bracket.

• | Release the 4 clips.

3. Remove the liftgate garnish molding - right side.

• | Remove the luggage shade bracket.

• | Release the 4 clips.

4. Lower the headlining. Refer to Headlining Trim Panel Replacement .
5. Remove the hose up to the liftgate boot.

Disconnect the wiring harness plug (1).

6. Expose the hose.

• | Remove the boot (1) at the liftgate.

• | Expose the washer/wiper system hose.

• | Cut the duct tape at (2, 3).

7. Disconnect and remove the hose.

• | Disconnect the hose at the center pillar (1).

• | Remove the hose.

• | Release the 5 clips (2, 3).

Important: Fasten new hose to old hose with adhesive tape.

8. Remove the hose.

Pull the new hose with the old hose.

### Installation Procedure

1. Route and connect the hose.
2. Install the headlining. Refer to Headlining Trim Panel Replacement .

Notice: Refer to Fastener Notice in the Preface section.

3. Install the liftgate garnish molding - right side.

• | Install the 4 clips.

• | Fasten the luggage shade bracket.

4. Install the liftgate garnish molding - left side.

• | Install the 4 clips.

• | Fasten the luggage shade bracket.

5. Connect the battery.
6. For reprogramming procedures, refer to Control Module References .