For 1990-2009 cars

### Removal Procedure

1. Open the sunshade.
2. Open the sunroof to the vent position.
3. Remove the rear window.

3.1. | Push up on the side covers to access the screws.

3.2. | Remove the 4 screws.

4. Remove the rear window.

### Installation Procedure

Important:

• | Tighten the rear window in the upper position.

• | Install the position window pane with the curve facing down.

1. Insert the rear window.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the rear window.

Align the rear window gap 1.5-2 mm (0.06-0.08 in).

Tighten
Tighten the 4 screws to 4 N·m (35 lb in).

3. Close the sunroof rear window.
4. Close the sunshade.