For 1990-2009 cars

## Luggage Shade Retainer Replacement Coupe

### Removal Procedure

1. Remove the door sill plate.

• | Release the 5 clips.

• | Remove the door sill inner plate (1).

2. Remove the luggage shade.

• | Disconnect the 2 retaining cords from the liftgate (arrows).

• | Pull out 2 covers from the side supports (1).

3. Remove the rear compartment carpet (1).
4. Remove the trailer hitch ball head.

• | Loosen the fastening belt (1).

• | Remove the ball head (2).

5. Remove the additional storage tray under the load compartment carpet.
6. Remove the rear compartment sill plate.

Release the 7 clips (1).

7. Remove the bench seat.

• | Disconnect the 2 front brackets (1).

• | Support the 2 bench seats from the rear bracket.

• | Push the seat simultaneously backwards and upward.

8. Remove the rear seat backrest (l).

• | Remove the 4 bolts (2) at the front.

• | Remove the 3 belt buckles (1).

• | Fold down the rear seat backrest (II).

• | Remove the 4 rear bolts (2).

9. Remove the rear seat backrest.
10. Remove the upper center pillar trim.

• | Pull out the plastic rivet (1) from the center pillar trim.

• | Remove the molding from the seat with a plastic wedge.

• | Remove the seat belt bolts (3).

• | Remove the cap (2).

• | Remove the upper center pillar trim.

11. Remove the rear quarter lower trim panel.

• | Remove the lower seat belt fastening (3).

- | Remove the lower seat belt anchor bar (4).

- | Remove the seat belt with striker.

- | Remove the seat belt striker guide bushing (5) from the rear quarter panel front.

• | Remove the rear quarter panel cover cap (2).

• | Remove the bolt.

• | Remove the bolt (6) from the rear seat backrest.

• | Remove the bolt (1) from the upper center pillar.

• | Release the lower rear quarter panel trim.

• | Remove the 8 clips (7).

12. Remove rear compartment side trim.

• | Remove the 3 bolts (1) from side load compartment cover.

• | Release the 2 clips (3).

• | Disconnect the luggage compartment light wiring harness plug (2).

• | Remove the rear compartment side trim.

13. Remove the left side upper quarter trim panel.

• | Remove the upper quarter trim seat belt fastening screws.

• | Remove the cover cap (1).

• | Release the 3 C-pillar upper quarter trim clips.

14. Remove the luggage shade retainer for the luggage shade.

• | Rotate the luggage shade retainer (1) 180 degrees.

• | Press out the luggage shade retainer from the outside inwards.

### Installation Procedure

1. Install the luggage shade retainer for the luggage/shade.

• | Press in the luggage shade retainer from the inside outwards.

• | Rotate the luggage shade retainer socket 180 degrees.

• | Bolt the luggage shad retainer lock.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the rear inner paneling, rear quarter panel.

• | Connect the luggage compartment light wiring harness plug.

• | Insert the rear compartment side trim.

• | Install the 2 clips.

Tighten
Tighten 3 bolts in the luggage shade side to 2.5 N·m (22 lb in).

3. Install upper left side quarter trim panel.

• | Install the 3 quarter trim panel clips.

Tighten
Tighten the quarter trim seat belt bolts to 35 N·m (26 lb ft).

• | Install the cover cap.

4. Install the rear quarter lower trim panel.

• | Install the 8 rear quarter panel clips.

Tighten

• | Tighten the bolt on the upper quarter trim panel to 2.5 N·m (22 lb in).

• | Tighten the bolt to the rear seat backrest to 40 N·m (30 lb ft).

• | Tighten the lower quarter trim panel bolt to 35 N·m (26 lb ft).

• | Install the rear quarter panel cover cap front.

• | Install the seat belt striker guide bushing to the rear lower quarter panel front.

• | Install the seat belt with striker

• | Install the lower seat belt striker

Tighten
Tighten the lower seat belt bolt to 35 N·m (26 lb ft).

5. Install the upper center pillar trim.

• | Guide the center pillar trim from above in inner paneling guide front of rear lower quarter panel.

• | Install the upper center pillar trim.

• | Press in the expanding bolt.

Tighten
Tighten the seat belt bolt to the center pillar trim to 35 N·m (26 lb ft).

• | Install the cover cap.

6. Insert the rear seat backrest.
7. Install the rear seat backrest.

• | Guide in and position the rear seat backrest with guide pins right and left in the rear quarter panel.

Tighten
Tighten the 4 rear bolts to 20 N·m (15 lb ft).

• | Fold down the rear seat backrest.

• | Insert the 3 belt buckles.

Tighten
Tighten the 4 front bolts to 35 N·m (26 lb ft).

8. Install the bench seat.

• | Support the 2 seats in the rear bracket.

• | Push the seat simultaneously backwards and down.

• | Bolt the 2 front brackets.

9. Install the rear compartment sill plate.

Install the 7 clips.

10. Install the additional storage trays under the load compartment carpet.
11. Install trailer hitch ball head.

• | Thread the belt through the eye.

• | Insert the ball.

• | Tighten the belt.

12. Install the rear compartment carpet.
13. Install the luggage shade.

• | Engage 2 covers in supports, side.

• | Attach the 2 retaining cords to the liftgate.

14. Install the sill inner paneling.

Install the 5 clips.

## Luggage Shade Retainer Replacement Sedan

### Removal Procedure

1. Remove the rear seat.

• | Disconnect at the loop (1) and support in rear area (arrow).

• | Remove the rear seat upwards.

2. Remove the rear seat backrest.

• | Remove the 3 bolts at the front.

• | Remove the 3 belt buckles.

• | Fold down the rear seat backrest.

• | Remove the 3 bolts at the back.

3. Remove the rear seat backrest.

Remove the rear seat backrest from the side guide.

4. Remove the lower quarter trim panel.

Release the 3 clips (arrows) and remove.

5. Remove the seat belt on lower quarter trim panel.

Remove the bolt.

6. Remove the upper quarter trim panel.

• | Release the access panel (1).

• | Release the upper quarter trim panel.

• | Release the 5 clips.

• | Unthread the seat belt.

• | Remove the upper quarter trim panel.

7. Remove the rear compartment sill panel.

• | Release carefully in the upper area (2) with a plastic wedge.

• | Release the 4 clips.

• | Release in the lower area in the direction of the interior.

• | Release the 4 clips.

8. Remove the rear quarter trim panel.

• | Remove the 3 bolts (1).

• | Disconnect the wiring harness plug.

• | Loosen 3 clips.

• | Remove the quarter trim panel.

9. Remove the luggage shade retainer (1).

### Installation Procedure

1. Install the luggage shade retainer.

Insert and install the luggage shade retainer.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the rear quarter trim panel.

• | Connect the wiring harness plug.

• | Install the 3 clips.

Tighten
Tighten the 3 bolts to 2.5 N·m (22 lb in).

3. Install the rear compartment sill trim.

Install the 8 clips.

4. Install the upper quarter trim panel.

• | Thread in seat belt.

• | Install the upper quarter trim panel.

• | Install the panel.

5. Install the seat belt.

Tighten
Tighten the bolt to 35 N·m (26 lb ft).

6. Install the lower quarter trim panel.

Install the 3 clips.

7. Insert the rear seat backrest.

Insert the rear seat backrest into side guide.

8. Install the rear seat backrest.

Tighten
Tighten the 3 rear bolts to 20 N·m (15 lb ft).

• | Tighten the 3 rear bolts.

• | Fold down the rear seat backrest.

Tighten
Tighten the 3 front bolts with seat belt buckle to 35 N·m (26 lb ft).

9. Install the rear seat.

Insert the rear seat cushion and position.