For 1990-2009 cars

### Removal Procedure

1. Remove the panel for the microphone (2) and the panel for the sliding sun roof control unit (3).

Release using a suitable tool (screwdriver).

2. Release the lens from the interior lamp (1).
3. Remove the front interior lamp holder.

• | Remove the 2 bolts (1).

• | Release the holders (4) all around.

• | Release the wiring harness holder (2).

• | Disconnect the wiring harness plug (3).

4. Remove the microphone.

• | Disconnect the compact plug (1).

• | Release and disconnect the wiring harness at the compact plug (arrow).

• | Disconnect and remove the microphone (2).

### Installation Procedure

1. Install the microphone.

• | Install in the microphone.

• | Connect the wiring harness plug.

• | Connect the compact plug.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the interior lamp holder.

• | Install the 4 retaining lugs.

Tighten
Tighten the 2 screws to 2.5 N·m (22 lb in).

• | Connect the wiring harness plug into the holder.

• | Connect and lock the 2 wiring harness plugs.

3. Install the panel for the sunshade actuation switch.
4. Install the microphone cover.
5. Install the lens for the front interior lamp.