For 1990-2009 cars

### Removal Procedure

1. Tilt the steering column in the upper position.
2. Remove the light switch center.

2.1. | Turn the light switch (1) to the left position and press in, then turn pressed switch to the middle position (3).

2.2. | Remove the light switch center (2).

3. Remove the inner paneling for the driver side knee bolster.

3.1. | Remove the 4 bolts.

3.2. | Disconnect and remove the driver knee bolster from the bracket.

### Installation Procedure

1. Install the inner paneling for the driver side knee bolster.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the driver knee bolster into the lower bracket.

Tighten
Tighten the 4 bolts to 2.5 N·m (22 lb in).

3. Install the light switch center.

3.1. | Connect and latch the wiring harness plug.

3.2. | Insert the light switch center.

3.3. | Turn the switch to the OFF position.

3.4. | Tilt the steering column downwards.