For 1990-2009 cars

### Removal Procedure

Note: Always perform adjustment at both tie rods. The two tie rods may display a maximum difference in length of 5 mm (0.20 in) after adjustment.

1. Put the steering in straight ahead position.
2. Loosen the lock nut (1) at left and right tie rods.

Counterhold at tie rod using open-ended wrench.

3. Adjust the wheel toe by rotating the tie rod (2).

Note: The nominal value includes a tolerance range, thus permitting a toe-in setting (+ wheel toe) as well as a toe-out (- wheel toe). The tie rods must be set so that either both front wheels point inwards by half of the front toe-in setting, or both front wheels point outwards by half of the front toe-out setting.

4. For specifications, refer to Wheel Alignment Specifications.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

Note: Ensure that the boot on the steering gear is not twisted.

1. Tighten the lock nuts on both tie rods.

Counterhold at the tie rod using open-ended wrench.

Tighten
Tighten the lock nuts to 60 N·m (44 lb ft).

Note: The steering wheel must be in the straight-ahead position when inspecting by means of a test drive.

2. Inspect the wheel toe adjustment.