For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle.
2. Remove the fascia. Refer to Front Bumper Fascia Replacement .
3. Remove the auxiliary fan (1).

• | Disconnect the cable ties.

• | Unclip the relays.

• | Disconnect the wiring harness connector.

• | Detach the wiring harness.

• | Unclip the clips.

• | Remove the nuts.

• | Pull the auxiliary fan from the bracket and remove from below.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the auxiliary fan.

• | Insert the auxiliary fan housing into the bracket

Tighten
Tighten the nuts to 5 N·m (44 lb in).

• | Attach the wiring harness.

• | Clip in the clips.

• | Fix the wiring harness plug.

• | Clip in the relays.

• | Attach the cable ties.

2. Install the front fascia. Refer to Front Bumper Fascia Replacement .
3. Lower the vehicle.